{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Table 1"],"read":"whole","date_system":"1900"}

{"sheet":"Table 1","index":0,"n_rows":17,"n_cols":9,"rows_kept":17,"merged":[[0,0,0,8],[1,0,1,8],[3,1,9,1],[7,3,9,3],[11,1,13,1],[15,2,15,8],[16,0,16,8]]}
["合肥体育中心游泳馆比赛检录区等场地搭建需求清单"]
["项目概况：\n1.整体施工区域1400㎡：需做好场地、地面等保护措施，必须使用PVC防火地保板，1.5cm多层板；\n2.跳水池面积525㎡；泳池尺寸：25×21×6m；\n3.周边区域面积：775㎡；"]
["序号","区域","名称","参数","数量","单位","单价\n（元）","合计\n（元）","说明"]
[4,"跳水池\n垫层区搭建","跳水池下层地面保护版","1.5cm多层板",525,"平方",null,null,"符合防火要求"]
[5,null,"立柱杆","材质为Q345B\n管直径为φ48mm,管壁厚为3.2mm",null,"根",null,null,"符合材质要求"]
[6,null,"横杆","材质为Q235\n管直径为φ48mm,管壁厚为3.2mm",null,"根",null,null,"符合材质要求"]
[7,null,"斜拉杆","材质为Q235\n管直径为φ48mm,管壁厚为3.2mm",null,"根",null,null,"符合材质要求"]
[8,null,"扁梁杆","定制款\n（规格、型号、尺寸、材质等必须与5.6.7项设施匹配）",null,"根"]
[9,null,"卡托",null,null,"个"]
[10,null,"四爪扣",null,null,"个"]
[11,"周边区域\n搭建","定制方盒","区域面积：775㎡；\n尺寸：20cm*30cm*30cm",null,"个",null,null,"需防火涂料粉刷，符合防火要求"]
[12,"整体区域\n搭建","补充平台板","1220mm*2440mm*18mm，钢结构+阻燃板\n环保阻燃胶合板，燃烧性能B1(C）级",1300,"平方",null,null,"符合防火要求；整体区域找平，平整度落差不大于5mm；"]
[13,null,"多层板","2cm多层阻燃板",1300,"平方",null,null,"符合防火要求"]
[14,null,"阻燃地毯","圈绒蓝色，厚度为5mm\n符合GB 20286-2006",1300,"平方",null,null,"符合防火要求"]
[15,"台阶","定制台阶","阻燃木制,圈绒蓝色地毯包装，厚度为5mm，台阶边缘需做圆滑处理\n（符合GB 20286-2006）",4,"个",null,null,"符合材质要求；尺寸及踏步数需现场测量"]
[16,"总价（元）"]
["注：\n1、本工程主体采用layher钢架结构，规格为2.44m*2.44m方体，立柱每层高度为1.5m，斜拉杆步距2.8m。底角采用螺丝脚调节水平，底角下方垫一层20cm*20cm*2cm厚钢板。安装方式为标准件插销式；\n2、layher 每格宽2米*深2米*高2米，4面均有斜拉；\n3、本项目需现场查勘、测量详细数据并签到，报价需同时提供具体施工设计方案。联系人：陈工13955191036；\n4、本项目施工时间为4天（8月15日-18日），施工完成后乙方需组织、甲方、施工方及相关专家进行验收，验收合格后经相关专家需签署意见并出具合法有效验收报告；\n5、请开具增值税专用发票，并标注开票税率（）%；\n6、报价包含但不限于运输、拆除、安装、施工、辅材、安全防护保险、质保等费用；\n报价单位（盖章）：                                                              联系方式："]